AGF Model 7600 Universal 3-Way Guage Valve

2.1 TRIM AND DRAIN VALVES

* + - * 1. General Requirements:

Standard: UL's "Fire Protection Equipment Directory" listing or "Approval Guide," published by FM Global, listing.

Pressure Rating: 300 psig minimum.

* + - * 1. Globe Valves:

Manufacturers: Subject to compliance with requirements, available manufacturers offering products that may be incorporated into the Work include, but are not limited to, the following:

AGF Manufacturing, Inc.; Model 7600.

<**Insert manufacturer's name**>.

3-way Globe Valve:

Conforms to NFPA standards NFPA-13, NFPA-13R and NFPA-13D.

Bronze body and stem.

1/4” NPT inlet and outlet connections.

1/4” test/drain port with a plug to facilitate draining of valve/gauge assemblies.