Model 5300A COLLECTanDRAIN

2.1 SPRINKLER SPECIALTY PIPE FITTINGS

* + - * 1. Auxiliary Drain and Condensation Collecting Assemblies for Dry Pipe and Preaction Sprinkler Systems:

Manufacturers: Subject to compliance with requirements, available manufacturers offering products that may be incorporated into the Work include, but are not limited to, the following:

AGF Manufacturing Inc.; Model 5300A COLLECTanDRAIN™.

<**Insert manufacturer's name**>.

Standards:

UL's "Fire Protection Equipment Directory" listing or "Approval Guide," published by FM Global, listing.

NFPA 13 and NFPA 25.

Components:

Two 1 inch MIPT x FIPT Brass quarter turn ball valves with chrome plated balls.

Two 1 inch by 2 inch Galvanized Bell Reducers.

2 inch by 12 inch Condensate Nipple.

1 inch Galvanized Square Head Plug.