PURGENVENT Model 7910MAV

2.1 AIR VENTING VALVES

* + 1. Series: PURGEnVENT as manufactured by AGF Manufacturing, Inc.
			1.

Product: Model M7910MAV. Manual Air Venting Valve is a 1/2 inch (13 mm) ball valve with a mesh strainer and ball float.

Standard: UL's "Product iQ" . NFPA 13, 13R, 13D (as applicable).

Pressure Rating: 300 psig (2070 kPa).

Body Material: Forged brass body.

Components: Stainless steel inlet screen (60 mesh), polypropylene float,

Inlet Size: 1/2 inch (13 mm) NPT.

Outlet Size: 1/2 inch (13 mm) NPT.